(footprint "ISP1807-edit"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Insight SiP BLE module all pins")
	(property "Reference" "REF**"
		(at 4.000005 -0.95 0)
		(layer "F.SilkS")
		(uuid "23351062-97ea-49a6-8913-be1bbab9602b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "ISP1807-edit"
		(at 4.000005 9.20001 0)
		(layer "F.Fab")
		(uuid "bf2b8096-df10-4458-a5f1-f227d20bc456")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "1975f96b-cec8-448d-aec8-0d6e14d034eb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "92897de2-6a65-44bd-b86e-b1811f0b1787")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_line
		(start 3.5 5.5)
		(end 4.5 5.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "Eco2.User")
		(uuid "50e5812a-1597-4061-9401-c6c55a423aac")
	)
	(fp_line
		(start 4 6)
		(end 4 5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "Eco2.User")
		(uuid "ad911f01-ab54-48bd-a9ce-083d76a74268")
	)
	(fp_line
		(start 0 0)
		(end 8 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "B.Fab")
		(uuid "02f28dc5-9d57-4801-95db-abd0bc8a36cc")
	)
	(fp_line
		(start 0 8)
		(end 0 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "B.Fab")
		(uuid "6a897964-5e98-4e2e-9981-08c7e3e8bc7c")
	)
	(fp_line
		(start 0 8)
		(end 8 8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "B.Fab")
		(uuid "e6b2d8b6-b945-430c-b3b9-b78a2dd5fda0")
	)
	(fp_line
		(start 8 8)
		(end 8 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "B.Fab")
		(uuid "8ba706ec-823d-4108-80b9-50158fe85cac")
	)
	(pad "1" smd rect
		(at 0.5 0.5)
		(size 0.8 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "3ce88965-9c1f-4eb8-b499-e397a9cfe699")
	)
	(pad "2" smd rect
		(at 0.3 1.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "e5e6214e-486a-49b5-b261-dd2f0ed58ff9")
	)
	(pad "3" smd rect
		(at 0.95 1.725)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "bdde1ef1-a073-4aec-bb5b-a5368f261800")
	)
	(pad "4" smd rect
		(at 0.3 2.05)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "279a2ab0-ac45-48d9-9bac-a175776c650a")
	)
	(pad "5" smd rect
		(at 0.95 2.375)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "b96bf272-dae0-41df-a021-ac9d2b7b46f7")
	)
	(pad "6" smd rect
		(at 0.3 2.7)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "264c5844-c781-46ec-985a-a6c71c3f2f0c")
	)
	(pad "7" smd rect
		(at 0.5 3.6)
		(size 0.8 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "17f69ba7-1091-45d1-86ef-9329468c0edc")
	)
	(pad "8" smd rect
		(at 1.4 3.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "f1d44fa3-5ea7-4c32-b9ce-f3cc08d9af22")
	)
	(pad "9" smd rect
		(at 1.725 3.15)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "102cb2cb-37bb-409c-8329-cc67b1cc31fd")
	)
	(pad "10" smd rect
		(at 2.05 3.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "7ebb747b-2bc0-4499-8ce4-0e24e4741f81")
	)
	(pad "11" smd rect
		(at 2.375 3.15)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "a29fd14d-b2d2-45d4-a6a6-10c6c3e74fbe")
	)
	(pad "12" smd rect
		(at 2.7 3.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "e071d09d-44d4-410d-9f6f-5609c8570777")
	)
	(pad "13" smd rect
		(at 3.025 3.15)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "4fe3bc03-2384-44a1-bfdf-d7fc8c1e4ecf")
	)
	(pad "14" smd rect
		(at 3.35 3.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "1424983e-b2aa-40b3-a6c2-f65700333ee3")
	)
	(pad "15" smd rect
		(at 3.675 3.15)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "514791b3-8435-420e-86f9-39006e3733e8")
	)
	(pad "16" smd rect
		(at 4 3.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "c2c6873d-13d9-4475-aa5f-b52fa4fa212e")
	)
	(pad "17" smd rect
		(at 4.325 3.15)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "233023cd-30b3-43cb-b2b6-50132a62754e")
	)
	(pad "18" smd rect
		(at 4.65 3.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "36014d39-f291-4416-94d6-822b32b9e7f8")
	)
	(pad "19" smd rect
		(at 4.975 3.15)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "f7f782b3-88ea-40b4-aa28-f099c0a0519e")
	)
	(pad "20" smd rect
		(at 5.3 3.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "4c072c4b-8f8a-4e24-9a99-d99d0fa6dce0")
	)
	(pad "21" smd rect
		(at 5.625 3.15)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "33444e04-e21d-46ba-ba44-b48c627f5560")
	)
	(pad "22" smd rect
		(at 5.95 3.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "76be17f4-fa96-4382-81a8-a3b89b60e107")
	)
	(pad "23" smd rect
		(at 6.275 3.15)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "d250e280-0532-4b9b-8efc-0f73758d52d0")
	)
	(pad "24" smd rect
		(at 6.6 3.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "6098b1b0-d52a-4002-8624-34c4560902aa")
	)
	(pad "25" smd rect
		(at 7.5 3.6)
		(size 0.8 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "e4b1e164-d95b-4e68-9100-db21d5fd72e3")
	)
	(pad "26" smd rect
		(at 7.7 2.7)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "dba34bed-d34b-4ac8-b8bd-1de43072184a")
	)
	(pad "27" smd rect
		(at 7.05 2.375)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "2f0046f5-b009-4294-8215-7b58c31c05ce")
	)
	(pad "28" smd rect
		(at 7.7 2.05)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "7b42a78f-1d67-47bf-84a1-b8a15650502f")
	)
	(pad "29" smd rect
		(at 7.05 1.725)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "5f0bc892-a0ef-4b4e-8088-11ab61b2f1d2")
	)
	(pad "30" smd rect
		(at 7.7 1.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "cb75aaa2-6b60-458d-bb37-5f01859ecff2")
	)
	(pad "31" smd rect
		(at 7.5 0.5)
		(size 0.8 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "0e0573d0-a215-4060-99f3-cd274a5807dc")
	)
	(pad "32" smd rect
		(at 6.6 0.3)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "2144f4cb-7d2d-431c-b61b-481b21416dcc")
	)
	(pad "33" smd rect
		(at 6.275 0.95)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "f94c1887-9088-4e35-9c5a-b7518ead1f15")
	)
	(pad "34" smd rect
		(at 5.95 0.3)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "5acf2d63-fadd-4ba9-9dc8-151308dcf4f3")
	)
	(pad "35" smd rect
		(at 5.625 0.95)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "804d1c92-6f26-4fd3-b180-0f4ed7b252b2")
	)
	(pad "36" smd rect
		(at 5.3 0.3)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "44610544-d028-4768-8fc1-85fddec75668")
	)
	(pad "37" smd rect
		(at 4.975 0.95)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "9ecfa98b-c345-431e-9a66-12d05458be81")
	)
	(pad "38" smd rect
		(at 4.65 0.3)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "57f619d2-eac5-4bbf-bb41-f8c9093573df")
	)
	(pad "39" smd rect
		(at 4.325 0.95)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "bf63c2a1-a861-417e-8812-f00a828e381c")
	)
	(pad "40" smd rect
		(at 4 0.3)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "929b2276-6e60-412b-85c1-92602934db5b")
	)
	(pad "41" smd rect
		(at 3.675 0.95)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "2583c7be-785c-42e1-a26f-16efecbbf3cf")
	)
	(pad "42" smd rect
		(at 3.35 0.3)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "7944e6cd-9bfc-4804-a0be-99ae9f0d914e")
	)
	(pad "43" smd rect
		(at 3.025 0.95)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "1c01c4c9-bf4a-49d3-bd74-e1d1c547c287")
	)
	(pad "44" smd rect
		(at 2.7 0.3)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "e66bfa32-13bd-4cc9-a8ca-41f0b65549f0")
	)
	(pad "45" smd rect
		(at 2.375 0.95)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "e1873020-9151-46f0-a318-808cc0e8c18f")
	)
	(pad "46" smd rect
		(at 2.05 0.3)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "2a7e6b1e-abee-4283-b7ad-2326c0a532f8")
	)
	(pad "47" smd rect
		(at 1.725 0.95)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "88198032-33aa-4d4e-aeb0-dfe41f2b37da")
	)
	(pad "48" smd rect
		(at 1.4 0.3)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "0de31c89-0978-46f8-8c76-ca81cbc837ee")
	)
	(pad "65" smd rect
		(at 0.3 4.55)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "4f83e8ea-b1bf-41c2-a781-0f4fb1dc8f8d")
	)
	(pad "66" smd rect
		(at 0.3 5.55)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "a89b89b6-533f-43a8-8e99-1167394ecefe")
	)
	(pad "67" smd rect
		(at 0.3 6.55)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "62a286ae-0b63-45bb-a29e-5776f1940922")
	)
	(pad "68" smd rect
		(at 0.5 7.5)
		(size 0.8 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "e2332ad7-d103-4105-8c4f-b6ec2a81b658")
	)
	(pad "69" smd rect
		(at 1.5 7.7005)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "b1ba1e54-efe7-4499-b45c-97be70092327")
	)
	(pad "70" smd rect
		(at 2.5 7.7005)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "ac0f0ecf-36f4-4a76-a2ed-8b447e8e719c")
	)
	(pad "71" smd rect
		(at 3.5 7.7005)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "24d1cd95-452f-429e-b5ae-f9129f23865a")
	)
	(pad "72" smd rect
		(at 4.5 7.7005)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "288cd814-276e-4c34-bbb8-b038a32c8fe1")
	)
	(pad "73" smd rect
		(at 5.5 7.7005)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "695a5422-0ca1-4c6f-8325-6b3193886a46")
	)
	(pad "74" smd rect
		(at 6.5 7.7005)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "97272e7c-5f2b-42a4-a980-05cb045d3f1d")
	)
	(pad "75" smd rect
		(at 7.5 7.5)
		(size 0.8 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "1ca05769-b702-4f8d-b1e4-a173acf4b58d")
	)
	(pad "76" smd rect
		(at 7.7 6.55)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "3d115c76-778b-4620-ab23-73b5ce75e6b8")
	)
	(pad "77" smd rect
		(at 7.7 5.55)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "2be3c4f6-639c-401d-90a1-703d1e73c2ad")
	)
	(pad "78" smd rect
		(at 7.7 4.55)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "d72f4e78-a5e4-4de4-93cf-2d4a6c7e1b40")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(uuid "75f876be-d871-48c2-9525-6dcfac214b81")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 8.1 -0.1) (xy 8.1 4.05) (xy 16 4.05) (xy 16.00001 8.49999) (xy -8 8.50001) (xy -8 4.05) (xy -0.1 4.05)
				(xy -0.1 -0.1)
			)
		)
	)
	(embedded_fonts no)
)
