(footprint "nordic_npm1300-QEAA_qfn"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -3.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "91fad935-f917-4c97-b3bd-16655cd2dfe7")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "nordic_npm1300-QEAA_qfn"
		(at 0 3.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0259c5cf-6ee8-4cb2-b5d4-3165d0245e7b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "fe6ca8d3-4ffe-4ba9-821f-a51f64224ead")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1d602488-088b-491a-a087-ce65e787a625")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.6 2.6)
		(end -2.6 2.2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "d5a9c075-b55d-443c-b52c-5f2416a64f8f")
	)
	(fp_line
		(start -2.2 2.6)
		(end -2.6 2.6)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "5c24ef7e-0c64-4dd2-ab2b-d23e8d9bd0ea")
	)
	(fp_line
		(start 2.2 -2.6)
		(end 2.6 -2.6)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c191c031-ed16-4b2e-9323-f0d84b2a9979")
	)
	(fp_line
		(start 2.6 -2.6)
		(end 2.6 -2.2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "b47fdd38-c6ad-4eee-a15f-a98f4d737d7d")
	)
	(fp_line
		(start 2.6 2.2)
		(end 2.6 2.6)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "58d668f9-b7b2-4d18-8c65-8b40ff016061")
	)
	(fp_line
		(start 2.6 2.6)
		(end 2.2 2.6)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "15d2cca3-819f-4c24-a814-bbc42896e0dc")
	)
	(fp_circle
		(center -2.35 -2.35)
		(end -2.1 -2.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill yes)
		(layer "F.SilkS")
		(uuid "429fa97b-b695-467c-994e-af539934d354")
	)
	(fp_rect
		(start -2.7 -2.7)
		(end 2.7 2.7)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "51089fa5-ab06-4d40-9444-030c55d3f48e")
	)
	(fp_poly
		(pts
			(xy -2.5 2.5) (xy 2.5 2.5) (xy 2.5 -2.5) (xy -1.35 -2.5) (xy -2.5 -1.35)
		)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "User.1")
		(uuid "ada01509-cf90-4f8b-94d5-ceac872c1a63")
	)
	(fp_text user "${REFERENCE}"
		(at 0 3.4 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "b1c19d8a-e6db-4c8f-8c35-07e4e7d6b474")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -2.3 -1.75 270)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "64a99622-2d27-4fe6-bdfe-7fece3928b3a")
	)
	(pad "2" smd roundrect
		(at -2.3 -1.25 270)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "eefa444b-d4f4-401b-bb92-2726ba2eac36")
	)
	(pad "3" smd roundrect
		(at -2.3 -0.75 270)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "55fb092e-ef1e-48d3-8b35-e029d05fc2b9")
	)
	(pad "4" smd roundrect
		(at -2.3 -0.25 270)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "7676e070-b15a-4029-81e7-27bb9a7fd3ea")
	)
	(pad "5" smd roundrect
		(at -2.3 0.25 270)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "84de2fc6-577c-454c-a1b2-b6024b75e986")
	)
	(pad "6" smd roundrect
		(at -2.3 0.75 270)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "7a6abcca-3e42-4c72-9ea8-db7926002420")
	)
	(pad "7" smd roundrect
		(at -2.3 1.25 270)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "7807381d-a999-4eb3-918e-466becbc2d49")
	)
	(pad "8" smd roundrect
		(at -2.3 1.75 270)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "aa88e1f8-63bd-4414-a245-b00870111910")
	)
	(pad "9" smd roundrect
		(at -1.75 2.3)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "c0125658-cda8-4f50-b354-c82d2f893cae")
	)
	(pad "10" smd roundrect
		(at -1.25 2.3)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "583ad9aa-a9c2-4c0e-8e1e-9ccfe12f1e99")
	)
	(pad "11" smd roundrect
		(at -0.75 2.3)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "43a54700-e086-409f-9188-4bb19b37b21f")
	)
	(pad "12" smd roundrect
		(at -0.25 2.3)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "d89a8edc-114c-4c4a-966b-240dbb2b55c0")
	)
	(pad "13" smd roundrect
		(at 0.25 2.3)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "a5e6360b-e925-4e2a-af3b-ddf26bbd06c9")
	)
	(pad "14" smd roundrect
		(at 0.75 2.3)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "ec737321-351a-4885-b23b-cde127566710")
	)
	(pad "15" smd roundrect
		(at 1.25 2.3)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "67d10333-ad36-471d-a5d9-5124ba5cea79")
	)
	(pad "16" smd roundrect
		(at 1.75 2.3)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "fd3fbf8a-d388-47ca-a58f-f9b6493f16a9")
	)
	(pad "17" smd roundrect
		(at 2.3 1.75 270)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "7049e9fe-c34f-4b96-879d-f36e5c48c339")
	)
	(pad "18" smd roundrect
		(at 2.3 1.25 270)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "3b8384b1-62cb-4ac5-8fc2-dafd444de054")
	)
	(pad "19" smd roundrect
		(at 2.3 0.75 270)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "84f887e2-7a41-4a69-9939-c75c3ac603e5")
	)
	(pad "20" smd roundrect
		(at 2.3 0.25 270)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "ea65d309-828c-4635-8d46-a3145d4722f1")
	)
	(pad "21" smd roundrect
		(at 2.3 -0.25 270)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "1cd6d6ab-d23b-4b04-a11b-24b70133bd47")
	)
	(pad "22" smd roundrect
		(at 2.3 -0.75 270)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "5ebc7e77-1738-4914-adb1-ed54627a536d")
	)
	(pad "23" smd roundrect
		(at 2.3 -1.25 270)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "8cbbaea0-5bce-443b-8bbf-e340ebdee32c")
	)
	(pad "24" smd roundrect
		(at 2.3 -1.75 270)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "0f4e7cf9-24ff-45c9-af81-dd4b1b46363a")
	)
	(pad "25" smd roundrect
		(at 1.75 -2.3)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "2a531efd-b59b-41d5-93e4-b283e8706321")
	)
	(pad "26" smd roundrect
		(at 1.25 -2.3)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "8f783eba-bfa0-4ce7-b344-a26f8a74d1be")
	)
	(pad "27" smd roundrect
		(at 0.75 -2.3)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "c6366111-7f37-4ca5-aea1-30009df456bf")
	)
	(pad "28" smd roundrect
		(at 0.25 -2.3)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "184afd5c-e5eb-4f90-b70c-0e4ea553d520")
	)
	(pad "29" smd roundrect
		(at -0.25 -2.3)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "bf9337ae-09e9-4f66-824c-4b9b1bdae1eb")
	)
	(pad "30" smd roundrect
		(at -0.75 -2.3)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "9b7f8a6e-6971-420c-a353-c6a30f00be7b")
	)
	(pad "31" smd roundrect
		(at -1.25 -2.3)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "9eb00628-ae81-44cb-abc9-44e9202413a2")
	)
	(pad "32" smd roundrect
		(at -1.75 -2.3)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "60a18651-7ebf-4768-beb3-0ade83e8a85b")
	)
	(pad "33" smd roundrect
		(at 0 0)
		(size 3.5 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0)
		(chamfer_ratio 0.15)
		(chamfer top_left)
		(uuid "dd757527-1a71-4c47-92ed-b6b030144f7a")
	)
	(embedded_fonts no)
)
