(footprint "L_0806_2016Metric"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -1.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "4d8fa824-de26-4675-8ca7-c955bebdb571")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "L_0806_2016Metric"
		(at 0 1.8 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f6edb324-4456-4150-a072-e660a0cc88dc")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "751bb4d5-bc02-45fa-b98c-fe0e897db83f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "296de66a-e3c7-4b30-9750-6dea2a8c2ab6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -1 -0.8)
		(end 1 0.8)
		(stroke
			(width 0.03)
			(type solid)
		)
		(fill no)
		(layer "Dwgs.User")
		(uuid "29715399-95d1-4821-b0b8-00b4cf6a5c54")
	)
	(fp_rect
		(start -1.2 -1)
		(end 1.2 1)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "a414cf5a-b5b5-4fcb-bb92-14cc578069d9")
	)
	(fp_text user "${REFERENCE}"
		(at 0 1.7 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "939b056d-d919-409c-bcd9-cb8e7c85061c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -0.75 0)
		(size 0.5 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "ed1d4527-3e6e-46b9-b06d-af8eeb2bd005")
	)
	(pad "2" smd roundrect
		(at 0.75 0)
		(size 0.5 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "975505e1-18ed-4ad3-9034-eabf7ef29ce0")
	)
	(embedded_fonts no)
)
