(footprint "magnetic connector 01x02P"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -1 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "07151d37-e060-431e-946a-5cbc08608ae8")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "magnetic connector 01x02P"
		(at 0 4.9 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "37f7e0ce-7262-47c6-bb52-ada566714ce8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "12d10016-ad86-4379-995e-88c1c64c9b7c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4f24c776-a05a-46c1-8446-6274e3cc9aa2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_poly
		(pts
			(xy 6 -2) (xy -6 -2) (xy -6 2) (xy -2.5 2) (xy -2.5 4.5) (xy 2.5 4.5) (xy 2.5 2) (xy 6 2)
		)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "8c87e42d-8055-4ac6-955c-1125e60bedc7")
	)
	(fp_line
		(start -6 1)
		(end -5 1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "User.1")
		(uuid "576f1888-bbab-4daf-b1c4-775a59127e9c")
	)
	(fp_line
		(start 6 1)
		(end 5 1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "User.1")
		(uuid "e28194ae-e4ca-4844-aa92-e0b2f56ff8d8")
	)
	(fp_rect
		(start -6 -2)
		(end 6 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "User.1")
		(uuid "f849d25f-41d3-4d4b-b22c-c455eb3a6cd5")
	)
	(fp_rect
		(start -6 0)
		(end 6 2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "User.1")
		(uuid "fa0fb67e-ef7d-44ea-bc51-c79e54cbee07")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "c468399a-1b4d-4d4a-aa5a-fa7d247db194")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at -1.27 3.3)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e5e6765e-0e69-4a5b-a8ff-8675e7148272")
	)
	(pad "2" thru_hole circle
		(at 1.27 3.3)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "02ee18d4-6807-4f5f-b9fa-48dd6b746cb3")
	)
	(embedded_fonts no)
)
