(footprint "swd_pad"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -3 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "2fd6084f-3909-424d-92b1-3a51c0744659")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "swd_pad"
		(at 0 3 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "997ddc14-e506-42ab-9ea4-dbc79762bb9d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3aef3e9b-c675-43c9-b9f5-c337161e4033")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4418990b-2863-429d-b2c4-2f9b5a6de7e5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 3.2 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "87355d82-617e-441f-8e54-70fd7a28c4d8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -2.54 -1.27)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "fe2373af-d33c-4ae3-9906-ed8e93c7630b")
	)
	(pad "2" smd circle
		(at -2.54 1.27)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "27c32909-466c-4e0e-a112-43490c6fe89b")
	)
	(pad "3" smd circle
		(at 0 -1.27)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "5aac18c9-8c35-4308-bf57-590650ddbe84")
	)
	(pad "4" smd circle
		(at 0 1.27)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "78427d61-d5e3-4718-8325-862c69b59af9")
	)
	(pad "5" smd circle
		(at 2.54 -1.27)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "481fcc61-1935-4443-a2b1-5db256b22905")
	)
	(pad "6" smd circle
		(at 2.54 1.27)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "a318a685-f374-4951-8383-18939b187596")
	)
	(embedded_fonts no)
)
