(footprint "THD_0510-30CL-GF"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "FFC FPC 1x30")
	(property "Reference" "REF**"
		(at 0 -0.1 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "2049bee6-3c5b-4552-a7ad-0cda7a903359")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "THD_0510-30CL-GF"
		(at 0 2.6 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "48804083-d49f-4df7-b4d6-eaeefdb51b96")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1fdbcdb1-986f-4004-b822-e743b0b6cff2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c537e70a-bd43-4942-85ba-630e5a43420d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_poly
		(pts
			(xy -7.6 -2.1) (xy -8.6 -2.1) (xy -8.6 1.3) (xy -8 1.3) (xy -8 2.3) (xy 8 2.3) (xy 8 1.3) (xy 8.6 1.3)
			(xy 8.6 -2.1) (xy 7.6 -2.1) (xy 7.6 -2.8) (xy -7.6 -2.8)
		)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "93c6cc44-abba-450c-bb74-23651c56661f")
	)
	(fp_line
		(start -8.4 -1.9)
		(end 8.4 -1.9)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "User.1")
		(uuid "f33add3f-7a35-4884-9cbe-90066846a8ae")
	)
	(fp_line
		(start -8.4 -1.215)
		(end 8.4 -1.215)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "User.1")
		(uuid "58974559-68ca-4733-87b5-1f5d5c68162e")
	)
	(fp_line
		(start -8.4 -0.1)
		(end -8.4 -1.9)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "User.1")
		(uuid "e959a053-3788-4c86-b60e-69cc2c5b19e9")
	)
	(fp_line
		(start -7.8 1.4)
		(end -7.8 -0.4)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "User.1")
		(uuid "24717abc-4f39-4dd2-ad51-1ef3f93eb82b")
	)
	(fp_line
		(start 7.8 -0.4)
		(end 7.8 1.4)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "User.1")
		(uuid "4134daa8-cdc0-4a6a-a171-43b536d31a3f")
	)
	(fp_line
		(start 7.8 1.4)
		(end -7.8 1.4)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "User.1")
		(uuid "9f428684-8e45-4645-ba2d-da9e74868217")
	)
	(fp_line
		(start 8.4 -1.9)
		(end 8.4 -0.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "User.1")
		(uuid "788f8d0d-e48d-4938-8728-799a449d2596")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "aa3c21dd-a1f7-47ed-944c-0998b06ea8f1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -7.25 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "6c5cef19-6dea-43d8-8b5d-f542ee8ac7cb")
	)
	(pad "2" smd roundrect
		(at -6.75 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "2e43542f-3b4f-427b-a124-3b0a2d698e08")
	)
	(pad "3" smd roundrect
		(at -6.25 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "ae29666e-bb7d-486f-bfb6-2b624af34249")
	)
	(pad "4" smd roundrect
		(at -5.75 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "79b017ff-d22f-4c11-862c-7dce0e7b17dc")
	)
	(pad "5" smd roundrect
		(at -5.25 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "6a5064f9-f7de-40c3-b459-5964445a707b")
	)
	(pad "6" smd roundrect
		(at -4.75 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "20c50f0d-e047-413b-85ac-a7fec7a57840")
	)
	(pad "7" smd roundrect
		(at -4.25 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "6e1532ac-9852-49d9-9660-56a373c0f8f9")
	)
	(pad "8" smd roundrect
		(at -3.75 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "be589f40-79b9-4b3c-8d7c-8dc8f52b61ab")
	)
	(pad "9" smd roundrect
		(at -3.25 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "99d386ca-f641-41d3-b45c-9f791852baee")
	)
	(pad "10" smd roundrect
		(at -2.75 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "3bebd38a-6304-4463-9830-67dbb4767e5f")
	)
	(pad "11" smd roundrect
		(at -2.25 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "f41b93e3-9919-4b52-84f2-420d9db374e3")
	)
	(pad "12" smd roundrect
		(at -1.75 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "92b39fb5-e923-4b6b-af12-70b862a082c5")
	)
	(pad "13" smd roundrect
		(at -1.25 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "d4a26720-f452-410f-beff-603288916760")
	)
	(pad "14" smd roundrect
		(at -0.75 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "90be25c6-a0e3-48b2-9ea1-67c9d2e4c7c1")
	)
	(pad "15" smd roundrect
		(at -0.25 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "fc638f70-8d92-45e4-8216-2ee47ffbeb5f")
	)
	(pad "16" smd roundrect
		(at 0.25 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "7918ed30-5b86-4180-8dc8-a4c747e0299a")
	)
	(pad "17" smd roundrect
		(at 0.75 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "d11bd994-0eda-4715-95ef-d474b7f6ca6a")
	)
	(pad "18" smd roundrect
		(at 1.25 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "b3878f41-97f2-4392-b4c9-24dcc04f1871")
	)
	(pad "19" smd roundrect
		(at 1.75 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "f25786b3-30f9-43b0-a3a5-e3d2a19187dc")
	)
	(pad "20" smd roundrect
		(at 2.25 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "ac9c39a4-e5dd-493c-8ea1-c43b7ed076a8")
	)
	(pad "21" smd roundrect
		(at 2.75 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "ed15ad15-0e9d-4856-8efd-8c54fb73f7ea")
	)
	(pad "22" smd roundrect
		(at 3.25 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "064f871f-f210-4711-95e2-42cd00b9f06d")
	)
	(pad "23" smd roundrect
		(at 3.75 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "2e8cd066-535e-478a-b848-ec9adbbb4f68")
	)
	(pad "24" smd roundrect
		(at 4.25 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "b641f6d8-2aa9-4f2b-8799-714c87d943f0")
	)
	(pad "25" smd roundrect
		(at 4.75 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "b74d6277-0895-4993-bba7-a7fb51d16a74")
	)
	(pad "26" smd roundrect
		(at 5.25 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "4ea2715b-a09f-44e3-afec-8c05308644cb")
	)
	(pad "27" smd roundrect
		(at 5.75 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "e14d188b-652e-40b0-9704-53b92b23fc0d")
	)
	(pad "28" smd roundrect
		(at 6.25 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "871c4698-8f28-4fb6-8004-3f9e81860a2c")
	)
	(pad "29" smd roundrect
		(at 6.75 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "02cee3b9-6d4f-4ee2-b775-542489590517")
	)
	(pad "30" smd roundrect
		(at 7.25 -2.3)
		(size 0.3 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "845ed50e-10c8-4c0c-b86b-90b58959ca14")
	)
	(pad "MP" smd roundrect
		(at -8.135 0.51)
		(size 0.3 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "662f0ceb-dff7-4b23-a357-e3c2edccb081")
	)
	(pad "MP" smd roundrect
		(at 8.135 0.51)
		(size 0.3 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "ac2085e2-fad3-4e59-8560-bfc430733e5d")
	)
	(embedded_fonts no)
)
