(footprint "DFN2010"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -15.9 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "5724f42c-dc41-41a6-b892-236371cbbf99")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "DFN2010"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "824103ed-9521-4947-ba3a-91f59bf0f505")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7ecf45de-a410-4d35-aa8c-129b5eed0ea4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "61cb58d9-c37d-4e51-ba99-caa7ff47fd83")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.05 0.35)
		(end -1.05 0.55)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "0b84948a-de4a-461c-bb11-f2b27d1e287c")
	)
	(fp_line
		(start -1.05 0.55)
		(end -0.85 0.55)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "b739c0cd-336c-4a91-9aab-e56caad713bc")
	)
	(fp_line
		(start 0.85 0.55)
		(end 1.05 0.55)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "1bc11b0c-c94e-4edd-91fe-51a7ba0ad63b")
	)
	(fp_line
		(start 1.05 -0.55)
		(end 0.85 -0.55)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "ed57da15-b413-4a06-b42a-378f7fe4a3de")
	)
	(fp_line
		(start 1.05 -0.35)
		(end 1.05 -0.55)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "f02d0d49-7065-42dd-8475-561f1c515267")
	)
	(fp_line
		(start 1.05 0.55)
		(end 1.05 0.35)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "53a49f48-f7a9-4a4e-9e3d-dd574eeedc8b")
	)
	(fp_circle
		(center -1.05 -0.5)
		(end -1.05 -0.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill yes)
		(layer "F.SilkS")
		(uuid "5e5a7412-5a6b-4efa-8721-ea913a60325d")
	)
	(fp_rect
		(start -1.15 -0.65)
		(end 1.15 0.65)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "54a19540-9272-491d-9148-9e818395c3a9")
	)
	(fp_poly
		(pts
			(xy -1 0.5) (xy 1 0.5) (xy 1 -0.5) (xy -0.65 -0.5) (xy -1 -0.15)
		)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "User.1")
		(uuid "8c9dd4f4-17b3-4399-ab63-ee9f69ef5c0e")
	)
	(fp_text user "${REFERENCE}"
		(at 0 1.35 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "b809b262-e3ee-434b-9b2f-13481e63dde5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -0.8 -0.35)
		(size 0.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0)
		(chamfer_ratio 0.35)
		(chamfer bottom_left)
		(uuid "5bd93298-5dc8-4210-8fe3-3c8ebc6ee271")
	)
	(pad "2" smd rect
		(at 0 -0.35)
		(size 0.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "c4b1184d-644a-4886-9641-5b5e1e1999f9")
	)
	(pad "3" smd rect
		(at 0.8 -0.35)
		(size 0.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "e8ca90b0-3adf-425a-bbe5-be5c40ff65ed")
	)
	(pad "4" smd rect
		(at 0.4 0.35)
		(size 0.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "3a6a4c10-11ca-4ad8-94d3-490db7c60f5b")
	)
	(pad "5" smd rect
		(at -0.4 0.35)
		(size 0.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "ae4886c5-b999-4f4f-9661-9b19ac7598c5")
	)
	(embedded_fonts no)
)
